{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[2,0,4,0]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿洗煤厂建设项目第一批设备采购"]
["标号","设备名称","电机型号","技术特征","单位","数量","备注"]
["包一","破碎机"]
[null,"筛分车间大块原煤破碎机","\n75kW×2","1、齿辊间距≥750mm，齿辊长度≥2000mm；                        2、破碎量≥300TPH/台；           3、入料粒度300-90mm，排料粒度≤200mm","台",1]
[null,"主厂房块精煤破碎机","75kW×2","1、齿辊间距≥750mm，齿辊长度≥2000mm；                            2、破碎量≥400TPH/台，通过量≥600TPH/台；                         3、入料粒度200-30mm，排料粒度≤50mm","台",1]
["包二","主厂房重介浅槽分选机","22kW","1、槽体B=6700mm, 刮板宽1372mm, 刮板高254mm；                           2、人料200-6（10）mm；                            3、处理能力≥650t/h， 排矸能力≥230t/h","台",1]
["包三","旋流器",null,"1、φ450x3旋流器组，截留粒度0.25mm；                                   2、立式","组",1,"3台/组"]
["包四","弛张筛","75kW","1、3080型双层弛张筛；                         2、上层φ=30mm，下层φ=6（10）mm","台",2]
["包五","分级筛、脱泥筛、脱介筛"]
[1,"主厂房块煤脱泥筛","30kW","1、3048型单层直线筛，φ=3mm，5°倾角                                     2、入料粒度-90（200）mm，","台",2]
[2,"主厂房块精煤脱介筛","55kW","1、3673型双层香蕉筛；                  2、上层筛筛孔10mm，下层筛缝1mm","台",1]
[3,"主厂房块矸石脱介筛","37kW","1、2448型双层直线筛；                    2、上层筛筛孔10mm，下层筛缝1mm","台",1]
["包六","离心机"]
[1,"主厂房块精煤离心机","75kW","卧式振动离心机，筛篮直径1500mm,筛缝0.40mm","台",1,"进口组装"]
[2,"主厂房粗煤泥离心脱水机","75kW","卧式刮刀煤泥离心脱水机，筛篮直径1200mm, 筛孔0.35mm","台",1,"进口组装"]
["包七","弧形筛","0.8kw","B=1500mm，筛缝0.50mm，包角60°","台",2]
["包八","超高压压滤机及配套设备"]
[1,"主厂房煤泥超高压压滤机","33.8Kw","1、滤板1500mmX1500mm，滤室厚度62mm，滤饼102块。进料压力：1-1.4Mpa，压榨压力：4-10MPa；            2、功率：33.8Kw/660V（功率最终厂家定）；                                 3、产量：12t/次，每小时产量15吨；                               4、滤饼含水量：≤27%（可打成粉）；                                  5、厂家带配电柜和控制柜。","台",2]
[2,"主厂房煤泥超高压压滤机配套入料泵","132KW","1、流量：0-200立方/小时，扬程：0-140米；                      2、进口:DN125（最终厂家定  ）3、出口:DN80（最终厂家定）   4、功率：132Kw/660V（功率最终厂家定）                         5、厂家带变频配电柜和控制柜","台",2,"控制方式：变频器"]
[3,"主厂房煤泥超高压压滤机配套压榨泵","75kW","1、流量：400L/min（24m3/h)；  2、最大压力：10MPa；                3、功率：75Kw/660V（功率最终厂家定）                                    4、厂家带变频配电柜和控制柜","台",2,"控制方式：变频器"]
[4,"主厂房煤泥超高压压滤机配套煤泥环锤破碎机","250KW","1/处理能力：250t/h;                      2、功率250Kw/660V（功率最终厂家定）;                              3、入料粒度300-500mm，排料粒度≤13mm，粉状","台",1]
["包九","磁选机"]
[1,"主厂房块煤磁选机","4.5kW","φ914x2972mm，逆流单滚筒，背靠背布置","台",2,"2台/组"]
[2,"主厂房加介磁选机","3kW","φ914x1500mm，逆流单滚筒","台",1]
["包十","浓缩机及煤泥水自动加药装置"]
[1,"浓缩车间浓缩机",null,"直径24m，中心传动，液压自动提耙，全桥式","台",1]
[2,"主厂房阴离子凝聚剂加药装置","10.41kW","搅拌桶5000L,存储桶10000L","套",1]
[3,"主厂房阳离子絮凝剂加药装置","10kW","搅拌桶5000L,存储桶10000L","套",1]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}