{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":75,"n_cols":6,"rows_kept":75,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿洗煤厂建设项目第二批设备采购清单"]
["序号","设备材料名称","型号","单位","数量","备注"]
["包一","防爆型永磁带式除铁器","电压660V，功率5.5KW，适应带宽1200mm，适应带速≤5.8m/s","台",1]
["包二","给煤机"]
[1,"给煤机","处理能力（煤量）：300-800t/h•台","台",4,"其中2台要求变频"]
[2,"给煤机","处理能力（煤量）：800-1200t/h•台","台",1]
["包三","装车闸门、电液动三通分料器和平板闸门"]
[1,"矸石仓装车闸门","鄂式双扇装车闸门","套",2]
[2,"块煤装车点装车闸门","电液推杆扇形闸门","套",3]
[3,"三通分料器","主厂房块精煤溜槽318A三通分料器","套",1]
[4,"电液动双缸平板闸门","转载点末煤机头溜槽711A电液动双缸平板闸门","套",2]
[5,"三通分料器","块煤储煤场块煤筛分点块煤分级筛筛前溜槽732A三通分料器","套",1]
["包四","渣浆泵"]
[1,"323浅槽合介泵","流量1340m3/h，扬程24m，比重1.8，电压660V","台",1,"详见技术规格书参数要求"]
[2,"325块煤稀介泵","流量500m3/h，扬程38m，比重1.2，电压660V","台",1,"详见技术规格书参数要求"]
[3,"332加介泵","流量100m3/h，扬程18.5m，比重2，电压660V","台",1,"详见技术规格书参数要求"]
[4,"336重介系统清扫泵","流量60m3/h，扬程25m，比重1.2，电压660V","台",1,"详见技术规格书参数要求"]
[5,"337轴封水泵","流量45m3/h，扬程53m，比重1，电压660V","台",1,"详见技术规格书参数要求"]
[6,"362分级旋流器入料泵","流量500m3/h，扬程40m，比重1.2，电压660V","台",1,"详见技术规格书参数要求"]
[7,"376清水泵","流量30m3/h，扬程35m，比重1，电压660V","台",1,"详见技术规格书参数要求"]
[8,"854压滤系统清扫泵","流量60m3/h，扬程20m，比重1.2，电压660V","台",1,"详见技术规格书参数要求"]
[9,"压滤系统水封泵","流量4m3/h，扬程82m，比重1，电压660V","台",1,"详见技术规格书参数要求"]
[10,"612、613 浓缩机底流泵","流量300m3/h，扬程16m，比重1.2，电压660V","台",2,"详见技术规格书参数要求"]
[11,"块煤系统喷水泵","流量500m3/h，扬程46m，比重1，电压660V","台",1,"详见技术规格书参数要求"]
[12,"冲洗水泵","流量50m3/h，扬程80m，比重1，电压660V","台",1,"详见技术规格书参数要求"]
[13,"事故池转排潜污泵","流量150m3/h，扬程20m，比重1.2，电压660V","台",1,"详见技术规格书参数要求"]
[14,"清扫泵","流量12.5m3/h，扬程19m，比重1.1，电压660V","台",4,"详见技术规格书参数要求"]
[15,"清扫泵","流量30m3/h，扬程15m，比重1.1，电压660V","台",1,"详见技术规格书参数要求"]
[16,"清扫泵","流量20m3/h，扬程32m，比重1.1，电压660V","台",1,"详见技术规格书参数要求"]
[17,"清扫泵","流量20m3/h，扬程15m，比重1.1，电压660V","台",1,"详见技术规格书参数要求"]
["包五","起重设备"]
[1,"主厂房洗选系统电动双梁起重机","20/5t","台",1,"详见技术规格书参数要求"]
[2,"主厂房压滤系统电动单梁起重机","10t","台",1,"详见技术规格书参数要求"]
[3,"机修车间电动单梁起重机","5t","台",1,"详见技术规格书参数要求"]
[4,"电动葫芦","2t","台",12,"详见技术规格书参数要求"]
[5,"手拉葫芦","5t","台",2,"详见技术规格书参数要求"]
[6,"手动单轨小车","5t","台",2,"详见技术规格书参数要求"]
[7,"手拉葫芦","3t","台",2,"详见技术规格书参数要求"]
[8,"手动单轨小车","3t","台",2,"详见技术规格书参数要求"]
[9,"手拉葫芦","5t","台",2,"详见技术规格书参数要求"]
[10,"手动单轨小车","5t","台",2,"详见技术规格书参数要求"]
["包六","压风设备"]
[1,"双螺杆空气压缩机","0.85MPa，21m3/min，660V","套",1]
[2,"螺杆空气压缩机","1.25MPa，2.7m3/min，660V","套",1]
["包七"]
[1,"电子皮带秤","B=800mm   ≤±0.25％","台",3,"防爆"]
[2,"电子皮带秤","B=1000mm  ≤±0.25％","台",2,"防爆"]
[3,"电子皮带秤","B=1200mm  ≤±0.25％","台",2,"防爆"]
["包八","采制样系统"]
[1,"中部采制样系统",null,"套",3]
["包九","电子汽车衡","3.4×21m-120t，4节","台",3]
["包十","搅拌器",null,"套",1]
["包十一","带式输送机"]
[1,"原煤带式输送机","B=1200mm，Q=947t/h，V=3.15m/s，L=86.575m，α=6~15°","套",1,"含带面"]
[2,"原煤带式输送机","B=1200mm，Q=947t/h，V=3.15m/s，L=59.8m，α=16°","套",1,"含带面"]
[3,"块煤带式输送机","B=1000mm，Q=520t/h，V=2.5m/s，L=251.6m，α=α=2-11-6.5-1.3°","套",1,"含带面"]
[4,"矸石带式输送机","B=1000mm，Q=350t/h，V=2.5m/s，L=144.6m，α=2-11-6.5°","套",1,"含带面"]
[5,"末煤带式输送机","B=1200mm，Q=900t/h，V=3.15m/s，L=88.35m，α=8-16°","套",1,"含带面"]
[6,"末煤上原混煤仓带式输送机","B=1200mm，Q=900t/h，V=3.15m/s，L=114.073m，α=15.8-11°","套",1,"含带面"]
[7,"末煤转载带式输送机","B=1000mm，L=27.65m，V=2.5m/s，倾角12-0°，Q=700t/h ","套",1,"含带面"]
[8,"块煤转载带式输送机","B=1000mm，L=26.65m，V=2.5m/s，倾角6°，Q=520t/h ","套",1,"含带面"]
[9,"矸石转载带式输送机","B=1000mm，L=18.35m，V=2.0m/s，倾角0°，Q=350t/h ","套",1,"含带面"]
[10,"煤泥转载皮带机","B=1200mm，L=20.30m，V=1.6m/s，倾角0°，Q=300t/h，正反转","套",1,"含带面"]
[11,"块煤带式输送机","B=1000mm，Q=520t/h，V=2.0m/s，L=28m，α=14-0°","套",1,"含带面"]
[12,"特大块煤带式输送机","B=800mm，Q=100t/h，V=2.0m/s，L=36.20m，α=0°","套",1,"含带面"]
[13,"中块煤带式输送机","B=800mm，Q=100t/h，V=2.0m/s，L=35.20m，α=0°","套",1,"含带面"]
[14,"小块煤带式输送机","B=800mm，Q=300t/h，V=2.0m/s，L=95.70m，α=0°","套",1,"含带面"]
[15,"小块煤带式输送机","B=1000mm，Q=600t/h，V=2.5m/s，L=81.6m，α=15-4°","套",1,"含带面"]
[16,"中块煤带式输送机","B=1000mm，Q=600t/h，V=2.5m/s，L=67.60m，α=15°","套",1,"含带面"]
[17,"大块煤带式输送机","B=1000mm，Q=600t/h，V=2.5m/s，L=73.60m，α=15-10°","套",1,"含带面"]
["包十二","刮板输送机"]
[1,"原煤配筛刮板输送机","B=1200mm，L=7.15m，V=0.96m/s，Q=947t/h","套",1]
[2,"末煤刮板输送机","B=1000mm，L=7.75m，V=0.85m/s  Q=500t/h ","套",1]
[3,"压滤机煤泥刮板输送机","B=1400mm，斜长L=14.8m，V=0.48m/s，Q=300t/h ，倾角3°","套",1]
[4,"配仓刮板输送机改造（延长2m）","B=1600mm,V=1.03m/s,L=64+2m Q=1800t/h,α=0°","套",2]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}