{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[5,5,9,5],[10,5,21,5]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿35KV变电站扩容项目设备采购清单"]
["序号","设备材料名称","型号","单位","数量","备注"]
["标段一","有载调压变压器","额定电压比：35±3×2.5%/10.5kV，变压器型号：SZ13-25000/35，变压器种类：油浸式","台",2,"详见技术规格书"]
["标段二","10kV箱式开闭所及35kV箱式变电站更换设备部分"]
[1,"10kV箱式开闭所",null,"套",1]
[1.1,"进线柜","KYN28A-12","面",2,"详见技术规格书，型号及供参考"]
[1.2,"母联及隔离柜","KYN28A-12","面",2]
[1.2999999999999998,"过电压抑制柜","AK-YZG","面",2]
[1.3999999999999997,"出线柜","KYN28A-12","面",14]
[1.4999999999999996,"交直流系统",null,"套",1]
[2,"35kV电流互感器","LZZBJ9-35\n500/5(0.2S/0.5/5P20/5P20，15/20/30VA)","组",6,"详见技术规格书"]
[3,"35kV电流互感器","LZZBJ9-35\n500/5(0.5/0.5/5P20/5P20，20/30VA)","组",9]
[4,"10kV带接地隔离开关","2000A-31.5kA","台",2]
[5,"10kV旋转式隔离开关","2000A-31.5kA","台",3]
[6,"10kV永磁式真空断路器","1600A-31.5kA DC220V","台",3]
[7,"电流互感器","LZZBJ9-10\n2000/5(0.2S/0.5/5P20/5P20，30/60/30VA)","组",6]
[8,"电流互感器","LZZBJ9-10\n2000/5(0.5/5P20，60/30VA)","组",3]
[9,"10kV带接地隔离开关","1250A-31.5kA","台",2]
[10,"10kV旋转式隔离开关","1250A-31.5kA","台",2]
[11,"电流互感器","LZZBJ9-10\n1200/5(0.5/5P20，20/20VA)","组",6]
[12,"零序电流互感器","LXK-∅240","台",2]
[13,"综合自动化系统",null,"套",1]
["标段三","10kV动态无功补偿装置","SVG-10kV/±2500kvar","套",2,"详见技术规格书"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}