{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":7,"rows_kept":3,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿工业场地门式起重机设备采购订货目录"]
["序号","设备名称","规格型号","技术参数","单位","数量","备注"]
[1,"门式起重机","双梁A型50/10t","1、额定起重量（t）：主钩50t/副钩10t\n2、跨度 ：24m\n3、电源（电压/频率）：380V/50Hz\n4、提升高度（轨面)：主钩10m/副钩11.1m\n5、工作级别：A5","台",1]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}